/**

\page Step06Page MITK Tutorial - Step 6: Use an interactive region-grower

The source is now split among several files:

\li Examples/Tutorial/Step6
\li https://www.mitk.org/download/tutorial-data/Pic3D.nrrd (image)

In this step the program is enhanced by the possibility to start a region-grower at interactively added points.
We will see how MITK images can be accessed as ITK images.
We now load the image file Pic3D.nrrd only since the surface will be the result of the region-growing.

Add points in the image by pressing SHIFT+left mouse key, then adjust the thresholds and press 'Start region growing'.

\imageMacro{step6_result.png,"",13.55}

The class Step6 inherits from QWidget and provides methods for setting up the widgets.
%Step6RegionGrowing.cpp contains a method for performing the region-growing. %Step6main.cpp contains main.
Like in ITK and VTK class member names start with m_ followed by the proper member name starting with a capital letter (e.g. m_Tree).
Function names start with capital letters. To learn more about style conventions in MITK read \ref StyleGuideAndNotesPage "The MITK Style Guide".

\dontinclude Step6.cpp

The widgets are initialized as in the previous steps but with an additional QVBox for a button to start the segmentation:

\skipline Create controlsParent
\until hlayout->addWidget(m_LineEditThresholdMax)


This creates a button to start the segmentation and its clicked() signal is connected to the method StartRegionGrowing():

\dontinclude Step6.cpp

\skipline QPushButton *startButton
\skipline connect(startButton

\section AccessMTIKImagesAsITKImagesSection Access MITK images as ITK images

ITK images are templated whereas mitk::Images are not. To use ITK filters with MITK images, we have to convert from MITK to ITK. To do so, first
define an access method, which is templated as an ITK image is:

\code
template<TPixel, VImageDimension>
MyAccessMethod(itk::Image<TPixel, VImageDimension>* itkImage)
{
...
}
\endcode

If you don't understand this template syntax, you should read any C++ text book. Understanding template syntax is crucial to successfully using ITK.

To call this templated method with an (untemplated) mitk::Image, you can use the AccessByItk macro from mitkImageAccessByItk.h. This macro checks for
the actual image type of the mitk::Image and does any necessary conversions. Look into "Modules / Adaptor classes" for more information.

\code
AccessByItk(mitkImage, MyAccessMethod)
\endcode

\dontinclude Step6RegionGrowing.txx

In this step our access method is called RegionGrowing() (defined in %Step6RegionGrowing.txx ):
\skipline template
\until } //RegionGrowing()

Additionally the access function has to be instantiated for all datatypes and two/three dimensions as some compilers have memory problems without this explicit instantiation, some even need instantiations in separate files for 2D/3D: \n
For 2D in %Step6RegionGrowing1.cpp :

\dontinclude Step6RegionGrowing1.cpp

\skipline InstantiateAccessFunctionForFixedDimension

... and for 3D in %Step6RegionGrowing2.cpp :

\dontinclude Step6RegionGrowing2.cpp

\skipline InstantiateAccessFunctionForFixedDimension

\dontinclude Step6.cpp

The method StartRegionGrowing() finally calls our access method RegionGrowing():
\skipline Step6::StartRegionGrowing
\until }

\section ConvertingITKMITKSection Converting ITK images to MITK images and vice versa

In some cases it is useful to simply convert between ITK and MITK images. The direction ITK to MITK is easy, since mitk::Image can handle most data types. The direction MITK to ITK is more critical, since ITK images have to be instantiated with a fixed pixel type and fixed dimension at compile time.

\li \code mitk::Image mitk::ImportItkImage(itk::Image<...>) \endcode
\li \code mitk::CastToItkImage(mitkImage, itk::Image<...>) \endcode


\section ConnectingMITKToVTKSection Connecting MITK images to VTK

Images are not converted or copied: The data array is just accessed via an encapsulating VTK object.

\li \code vtkImageData* mitk::Image::GetVtkImageData(int time = 0) \endcode

\section SurfacesMITKToVTKSection MITK Surfaces to VTK and vice versa

Again: not a conversion, just accessing.

\li \code vtkPolyData* mitk::Surface::GetVtkPolyData(int time = 0) \endcode

\li \code mitk::Surface::SetVtkPolyData(vtkPolyData*, int time = 0) \endcode


\ref Step05Page "[Previous step]" \ref Step07Page "[Next step]" \ref TutorialPage "[Main tutorial page]"

*/
